{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["技术要求","清单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[0,0,0,4],[4,0,4,1],[4,2,4,4],[5,0,5,4]],"flags":["formulas_cached_only"]}
["采购项目清单：铝合金升降机采购"]
["序号","项目名称","数量或规模","资金预算\n（万元）","资金来源"]
["1、","铝合金升降机采购","1套",9,"自筹"]
["合计",null,null,9]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：铝合金升降机采购                 \n                                                                                        二、项目用途说明：我院妇儿院区高空平台较多且高度较高，不方便日常清洁工作。另，妇儿院区门诊大厅照明灯具高度较高，无法进行日常维护和维修工作，因此需要购置铝合金升降机1套。\n                                                                                       三、配置规格、附件及零配件（包括专用工具）：详情见后附清单\n            \n                                                                                                             \n四、详细技术要求、参数及产品资料等：技术要求及功能参数如下：①、税务登记证、营业执照、组织机构代码或三证合一的营业执照；②、法人签字并加盖公章的委托书；③、投标人的身份证及复印件；④、失信被执行人、重大税收违法案件当事人名单、政府采购严重违法失信行为记录名单查询记录（“信用中国”及“中国政府采购网”查询记录）；⑤、近三年内参加招投标活动在经营活动中没有重大违法违纪记录的书面声明；⑥、安全生产许可证。开标时，投标企业需提供上述证件的原件或复印件加公章由评委审验。                                   \n\n                                                                                                                                                                                                                                                                                                                \n五、售后服务条件及交货日期（或工期）：质量承诺（包括质保期及质保金）\n"]

{"sheet":"清单","index":1,"n_rows":38,"n_cols":4,"rows_kept":38,"merged":[[0,0,0,3],[1,0,1,3],[2,2,2,3],[3,0,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,0,12,3],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,0,21,3],[24,0,24,3],[25,1,25,3],[26,1,26,3],[27,1,27,3],[28,1,28,3],[29,1,29,3],[30,1,30,3],[31,1,31,3],[32,0,32,3],[33,0,33,3],[34,0,34,3],[35,0,35,3],[36,0,36,3],[37,0,37,3]],"flags":["formulas_cached_only"]}
["铝合金升降机招标技术规格"]
["一、技术要求"]
["序号","分类","要求"]
["技术规格参数"]
[1,"外形尺寸","≥3800*1450mm"]
[2,"台面尺寸","≥1500*950mm"]
[3,"额定承重","≥200kg"]
[4,"配用动力","整体模块式液压泵站"]
[5,"最大工作高度","≥21.7M"]
[6,"最大平台高度","≥20M"]
[7,"安全护栏高度","不低于1.1米"]
[8,"行走方式","半自动行走式"]
["设备材料参数"]
[1,"台面面板","铺≥4mm花纹钢板（要求具有防滑功能）"]
[2,"主梁","≥6.5厚高强度铝合金"]
[3,"电机","≥2.2KW"]
[4,"底架结构","100*100*4方管"]
[5,"液压油管","耐压32MPa双层钢丝网高压油管"]
[6,"密封件","进口品牌"]
[7,"油缸","缸径≥50mm"]
[8,"轮胎","400-8实心轮胎4只"]
["其它配置"]
[null,"紧急下降系统","倾斜保护系统","充电保护系统"]
[null,"紧急停止系统","故障诊断系统","油管防爆系统"]
["安全要求"]
[1,"升降平台在升降过程中自然偏摆量赢不大于0.5%的最大起升高度"]
[2,"在动力油路等出现故障时，应设置防止平台时失控下降的安全装置（允许有控下降）"]
[3,"平台上升至最大起升高度时，上升极限位置限制器应自动切断平台动力源"]
[3,"平台防护栏杆开口设计合理，防止人员误操作导致从开口出坠落。平台防护栏杆各结构件之间的最大空隙应不大于0.4㎡"]
[4,"当升降平台动力源切断时应设置紧急下降装置"]
[5,"平台上需设置控制按钮盒并明确标识功能"]
[6,"警告标识、程序注释、使用说明书"]
["其它要求"]
["1、为方便室内作业，设备自高不得超过2300mm。\n2、环温：设备应适合的环境温度范围为：-25℃～+50℃。\n3、湿度：设备应适合的环境湿度范围为：75％～95％ 。"]
["二、功能结构要求"]
["    主要结构件紧密焊接制造，钢结构件经严格的抛丸除锈表面处理，无任何焊接飞溅和焊渣。平台结构采用整体结构设计，表面采用高强度拉伸花纹板台面板，使平台具备良好的防滑性能。所有钢结构组件均经过两道底漆，两道面漆，且选用优质聚氨酯面漆和清漆，漆膜厚度不小于0.08mm，需烘干处理。"]
["三、电气要求"]
["    两相电压220V。控制电压DC24v。控制、按钮开关安装位置合理，便于操作，且各台设备操作台处均具备急停装置。不允许使用淘汰型号电机，设备使用的耗电设施均应该是节能产品或能效等级达到2级以上。"]