{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["技术要求"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[0,0,0,4],[4,0,4,1],[4,2,4,4],[5,0,5,4]],"flags":["formulas_cached_only"]}
["采购项目清单：中心院区视频监控存储扩容"]
["序号","项目名称","数量或规模","资金预算\n（万元）","资金来源"]
["1、","中心院区视频监控存储扩容","4T 270块，6T 110块\n硬盘录像机32路16盘位，24台；网线300米、插排12个等其他辅助材料",49,"自筹"]
["合计",null,null,49]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：中心院区视频监控存储扩容                 \n                                                                                        二、项目用途说明：增加监控存储时间为90天，达到相关要求。\n                                                                                       三、配置规格、附件及零配件（包括专用工具）：\n监控专用硬盘4T 270块，6T 110块\n硬盘录像机32路16盘位，24台\n机柜2个、网线300米、插排12个等辅助材料\n            \n                                                                                                             \n四、详细技术要求、参数及产品资料等：\n    硬盘参数：监控硬盘4TB 64MB 5900转 SATA 垂直 机械 PMR CMR，监控硬盘6TB 256MB 5400转 SATA 垂直 机械 PMR CMR \n    录像机参数： 3U标准机架式，2个HDMI，2个VGA,HDMI+VGA组内同源16盘位，可满配8T、10T硬盘 \n2个千兆网口     2个USB2.0接口、1个USB3.0接口\n1个eSATA接口    报警IO：16进8出\n支持RAID0、1、5、10，支持全局热备盘\n    软件性能：输入带宽：320M；32路H.264、H.265混合接入\n最大支持16×1080P解码\n支持H.265、H.264解码\n    Smart 2.0/整机热备/ANR/智能检索/智能回放/车牌检索/人脸检索/热度图/客流量统计/分时段回放/超高倍速回放/双系统备份                                   \n\n                                                                                                                                                                                                                                                                                                                \n五、售后服务条件及交货日期（或工期）：\n自开工日起15天之内完成。设备质保期2年，人为及不可抗力因素不在质保范围。\n"]