{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["技术要求","技术参数"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[0,0,0,4],[4,0,4,1],[4,2,4,4],[5,0,5,4]],"flags":["formulas_cached_only"]}
["采购项目清单：120专用车载信息终端采购"]
["序号","项目名称","数量或规模","资金预算\n（万元）","资金来源"]
["1、","120专用急救车载终端","6套",6,"自筹"]
["合计",null,null,6]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：120专用急救车载终端采购                 \n                                                                                        二、项目用途说明：\n                                                                                       三、配置规格、附件及零配件（包括专用工具）：见技术参数\n            \n                                                                                                             \n四、详细技术要求、参数及产品资料等：见技术参数                                  \n\n                                                                                                                                                                                                                                                                                                                \n五、售后服务条件及交货日期（或工期）：合同签订后15天内完成完成项目的安装与验收。\n"]

{"sheet":"技术参数","index":1,"n_rows":2,"n_cols":1,"rows_kept":2,"merged":[[1,0,3,0]],"flags":["formulas_cached_only"]}
["120专用车载信息终端技术参数"]
["核心模块CPU: MSM8937, 八核 （四核1.4GHz+四核1.1GHz） ROM: 16GB（EMMC） \nRAM: 2GB（DDR3） \n扩展内存:  支持TF卡, max 64GB \n显示屏：8寸 TFT-LCD，分辨率1280*720 \n触摸屏：触摸电容式，支持5点触摸 \n4G天线：内置，柔性天线 \n定位模块：定位方式GPS/北斗 \n工作电压：正常工作电压范围9V~16V \n工作电流：正常工作电流范围≤1.5A \n待机电流：(整机休眠模式） ≤2mA \n待机电流(8小时待命模式）≤30mA \n工作温度：工作温度范围-20℃~+70℃ \n存储温度：存储温度范围-30℃~+80℃ \n开机时间：冷启动 （断电开机）≤40S   \n热启动（待命开机）≤1S  \n地图：导航地图第三方导航（百度/高德）海量数据实时更新 \n系统：软件版本安卓6.0 \n升级方式：通过USB口 \n4G通信：移动：LTE B38/B39/B40；TD-SCDMA B34/B39；GSM B3/B8\n配套车载信息终端软件"]