{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["技术要求","清单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[0,0,0,4],[4,0,4,1],[4,2,4,4],[5,0,5,4]],"flags":["formulas_cached_only"]}
["采购项目清单：3号楼LED灯具采购（三次）"]
["序号","项目名称","数量或规模","资金预算\n（万元）","资金来源"]
["1、","3号楼LED灯具采购（三次）",1,16,"自筹"]
["合计",null,null,16]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：3号楼LED灯具采购（三次）                  \n                                                                                        二、项目用途说明：我院3号楼目前使用的内箱式灯具老化严重，灯罩面具发黄影响照明，为改善3号楼照明及节能效果，现需定制一批LED灯具，逐步对原有灯具替换改造\n                                                                                       三、配置规格、附件及零配件（包括专用工具）：1、具有履行合同所必需的设备和专业技术能力。2、具有良好售后服务能力。3、提供近期1—2份类似合同业绩。\n            \n                                                                                                             \n四、详细技术要求、参数及产品资料等：技术要求及功能参数如下：①税务登记证、营业执照、组织机构代码或三证合一的营业执照；②、法人签字并加盖公章的委托书；③、投标人的身份证及复印件；④、失信被执行人、重大税收违法案件当事人名单、政府采购严重违法失信行为记录名单查询记录（“信用中国”及“中国政府采购网”查询记录）；、近三年内参加招投标活动在经营活动中没有重大违法违纪记录的书面声明。⑥通过ISO9000质量管理体系认证。开标时，投标企业需提供上述证件的原件或复印件加公章由评委审验。\n\n                                                                                                                                                                                                                                                                                                                \n五、售后服务条件及交货日期（或工期）：质量承诺（包括质保期及质保金）\n"]

{"sheet":"清单","index":1,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[0,0,0,4],[5,0,5,4]],"flags":["formulas_cached_only"]}
["3号楼LED灯具采购清单"]
["序号","名称","规格型号","单位","数量"]
[1,"LED平面灯（20W）","1145mmx245mm","套",300]
[2,"LED平面灯（20W）","545mmx545mm","套",400]
[3,"LED平面灯（30W）","545mmx545mm","套",300]
["具体产品要求：\n1、平面灯外框要求使用散热系数大于1.2的铝合金框架，铝合金框架单壁厚度不小于1.2MM；平面灯整灯厚度≤9MM，最薄以满足功能及结构要求为准。\n2、平面灯整体发光为侧发光，要求发光均匀，不得有光斑、斑点及阴影等缺陷。  \n3、平面灯灯珠要求使用高光效高流明长寿命灯珠，整灯光效不小于100LM/W。\n4、平面灯灯珠数应满足40W可正常工作，电源功率可调，可根据现场需要将功率调整为如20W或30W等不同功率。\n5、平面灯属于平放式平面灯，应确保平放安装顺畅。\n6、产品设计寿命不少于五万小时，质保两年，终身维修。"]