{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["技术要求","配置要求"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":6,"n_cols":6,"rows_kept":6,"merged":[[0,0,0,5],[3,0,3,1],[4,0,4,1],[4,2,4,5],[5,0,5,5]],"flags":["formulas_cached_only"]}
["采购项目清单：生殖医院网络改造及网段规划采购"]
["序号","项目名称","数量或规模","资金预算\n（万元）","资金来源","备注"]
[1,"生殖医院网络改造及网段规划","1套",4.8]
["合计",null,null,4.8]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：生殖医院网络改造及网段规划1项           \n                                                                                                二、项目用途说明： 1、新购两台核心交换机：维也纳酒店楼层双核心连接中心医院本部。2、链路连接、网段规划部分：通过运营商双链路连接维也纳酒店及本部医院，达到两地互联互通效果，保证生殖医学中心系统平稳运行。\n                                                                                                三、配置规格、附件及零配件（包括专用工具）：1、机柜螺丝、扳手、螺丝刀，交换机、水晶头、扎带等；\n2、查线、贴线标、理线，标签机、标签纸等；\n3、交换机安装调试及售后\n            \n                                                                                                             \n四、详细技术要求、参数及产品资料等：配置要求见后附，品牌要求及其他：为了便于网络整体管理，新购交换机要求与中心医院本部核心交换机一致品牌。为保证工程质量及进度，投标人必须取得信息科出具的现场勘察证明。\n\n                                                                                                                                                                                                                                                                                                                \n五、售后服务条件及交货日期（或工期）：1、提供从硬件验收合格之日起，三年的免费质保服务，终身维护保修。\n2、提供7*24小时技术支持。\n3、 提供高效的服务，当系统出现故障后应可以在1小时内提供远程技术支持，故障严重或医院要求的情况下4小时内到达现场解决问题，并在12小时内完成故障处理工作。在12小时内无法解决的应提供同型号备机保障系统的正常运行。\n4、交货期为合同签署后30个日历天\n"]

{"sheet":"配置要求","index":1,"n_rows":9,"n_cols":3,"rows_kept":9,"merged":[[0,0,0,2],[8,0,8,2]],"flags":["formulas_cached_only"]}
["配置要求："]
["设备名称","数量","技术指标"]
["核心交换机","2台","1、交换容量≥598 Gbps、包转发率≥222 Mpps\n2、千兆电口≥24，光电复用口≥4，SPF接口≥2，SFP PLUS接口≥2，QSFP PLUS接口≥2.\n3、支持基于端口的VLAN、MAC的VLAN、协议的VLAN、IP子网的VLAN、QinQ，\n4、灵活QinQ、VLAN Mapping、Voice VLAN、GVRP\n5、支持DHCP Client、DHCP Snooping、DHCP Relay、DHCP Server\n6、支持OSPFv1/v2、OSPFv3、BGP4、BGP4+ for IPv6 、VRRP/VRRPv3、等价路由、策略路由\n7、支持ND（Neighbor Discovery）、IPv6-Ping，IPv6-Tracert，IPv6-Telnet，IPv6-TFTP、6to4 tunnel、支持ISATAP tunnel\n8、支持IGMP v1/v2/v3，MLD v1/v2、PIM-DM，PIM-SM，PIM-SSM、MSDP，MSDP for IPv6、MBGP，MBGP for IPv6 \n9、支持流镜像、支持端口镜像\n10、支持802.1X认证/集中式MAC地址认证、Guest VLAN、RADIUS认证、SSH 2.0、端口隔离、端口安全、PORTAL认证、DHCP Snooping、 BPDU guard， Root guard、支持uRPF(单播反向路径检测)、IP/Port/MAC的绑定功能\n支持VCT（Virtual Cable Test）电缆检测功能"]
["40KM万兆单模","4个","中心波长：≥850nm\n传输速率：≥10Gbps\n用户接口连接器类型：LC类型\n接口线缆规格：≥50/125µm\n最大传输距离：≥300M"]
["万兆多模","4个","中心波长：≥1550nm\n传输速率：≥10Gbps\n用户接口连接器类型：LC类型\n接口线缆规格：≥9/125µm\n最大传输距离：≥40KM"]
["光纤跳线","1批","LC-LC 2M万兆多模2对，LC-ST 2M单模1对，FC-ST 5M单模1对，FC-LC 5M单模1对，FC-LC 3M单模2对"]
["辅材","1批","水晶头、扎带、标签纸、RJ45,等"]
["安装调试及网段规划","1项","备安装、联调联试"]
["品牌要求及其他：为了便于网络整体管理，新购交换机要求与中心医院本部核心交换机一致品牌。为保证工程质量及进度，投标人必须取得信息科出具的现场勘察证明。"]