{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["技术要求","起搏器测试仪技术参数"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":8,"n_cols":6,"rows_kept":8,"merged":[[0,0,0,5],[3,5,4,5],[6,0,6,1],[6,2,6,5],[7,0,7,5]],"flags":["formulas_cached_only"]}
["采购项目清单：起搏器测试仪、立式灭菌器等医疗设备采购项目三次"]
["标段","项目名称","数量或规模","资金预算（万元）","资金来源","备注（规格）"]
["一标段","起搏器测试仪",1,9.5,"自筹"]
[]
[]
["合计",null,1,9.5]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：   起搏器测试仪、立式灭菌器等医疗设备采购项目   \n二、项目用途说明：                          \n三、配置规格、附件及零配件（包括专用工具）： \n                                                       \n                                                       \n                                                        \n四、详细技术要求、参数及产品资料等：\n  附技术偏离表、评分标准、产品彩页、相关证明文件      \n                                                          \n                                                             \n五、售后服务条件及交货日期（或工期）：\n   质保期≥2年                                          \n                                                        \n五、推荐供应商清单\n    一、除公开招标、单一来源外的其他院内采购方式，可推荐三家以上供应商，并且要具有可比性。\n    二、填写内容包括供应商名称、联系人、联系方式，产地、品牌或资质。\n推荐供应商1                                                \n                                                         \n推荐供应商2                                                \n                                                         \n推荐供应商3                                                \n                                                         \n推荐供应商4                                                \n                                                         \n推荐供应商5                                                \n                                                         "]

{"sheet":"起搏器测试仪技术参数","index":1,"n_rows":1,"n_cols":1,"rows_kept":1,"merged":[[0,0,10,1]],"flags":["formulas_cached_only"]}
["起搏器测试仪技术参数\n1、起搏频率：30-200ppm\n2、脉冲幅度：0.1-10.0V\n3、脉冲宽度：0.06-2.0ms\n4、感知灵敏度：0.5-20mV\n5、不应期：250ms\n6、开机默认参数：起搏模式：SSI，\n7、紧急起搏参数：起搏模式：SSI，\n屏幕显示：液晶显示屏\n1、具备起搏、感知、低电量指示灯\n2、大号屏幕显示数字\n3、*一键参数切换\n4、*大旋钮调试参数\n分析功能：\n1、*P/R波峰值测量：0.5mV-20.0mV，连续自动更新，可一键测试\n2、阻抗测量：可一键测试阻抗数值\n安全和电池：\n1、自检功能：开机自检，设备运行过程中不间断实时监控，具备系统异常保护功能\n2、安全性能：电除颤保护、静电保护，噪声反转，高频保护\n3、电池类型：两节AA型1.5V碱性干电池\n4、取出电池后的运行：不间断安全工作时间大于或等于一分钟\n5、具备测试安全锁"]