{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["技术要求","清单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[0,0,0,4],[4,0,4,1],[4,2,4,4],[5,0,5,4]],"flags":["formulas_cached_only"]}
["采购项目清单：扶梯清洗设备采购"]
["序号","项目名称","数量或规模","资金预算\n（万元）","资金来源"]
["1、","扶梯清洗设备采购","见清单",4.033,"自筹"]
["合计",null,null,4.033]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：扶梯清洗设备采购                 \n                                                                                        二、项目用途说明： 为做好妇儿院区扶梯设备日常清洁工作，现需购置扶梯清洗设备1套。\n                                                                                       三、配置规格、附件及零配件（包括专用工具）：详情见后附清单\n            \n                                                                                                             \n四、详细技术要求、参数及产品资料等：技术要求及功能参数如下：①、税务登记证、营业执照、组织机构代码或三证合一的营业执照；②、法人签字并加盖公章的委托书；③、投标人的身份证及复印件；④、失信被执行人、重大税收违法案件当事人名单、政府采购严重违法失信行为记录名单查询记录（“信用中国”及“中国政府采购网”查询记录）；⑤、近三年内参加招投标活动在经营活动中没有重大违法违纪记录的书面声明。开标时，投标企业需提供上述证件的原件或复印件加公章由评委审验。                                    \n\n                                                                                                                                                                                                                                                                                                                \n五、售后服务条件及交货日期（或工期）：质量承诺（包括质保期及质保金）\n"]

{"sheet":"清单","index":1,"n_rows":4,"n_cols":4,"rows_kept":4,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["扶梯清洗设备技术规格"]
["序号","物品名称","技术参数","采购数量"]
[1,"扶梯清洗机","清水箱≥ 6L \n污水箱≥ 3L \n滚刷直径≥ 120mm \n清洗宽度≥ 350mm \n动力源 220V/50HZ \n功率≥1200w \n刷压力 ≥19Kg \n工作噪音 ≤64db（A）\n设备长宽高方便扶梯清洁需要","1台"]
[2,"多功能抽吸机","清水箱≥ 10L \n污水箱≥ 9L \n吸力≥ 220mbar \n吸水功率≥1200w \n动力源 220V/50HZ \n喷雾压力≥ 2.4bar \n喷射流量≥30L/min\n空气流量≥50L/sec   \n设备长宽高方便扶梯清洁需要","1台"]