{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["技术要求","清单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[0,0,0,4],[4,0,4,1],[4,2,4,4],[5,0,5,4]],"flags":["formulas_cached_only"]}
["采购项目清单：医院供水主管道改造"]
["序号","项目名称","数量或规模","资金预算\n（万元）","资金来源"]
["1、","医院供水主管道改造","见清单",8.1795,"自筹"]
["合计",null,null,8.1795]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：供水主管道改造                 \n                                                                                        二、项目用途说明：医院南大门地下通道施工，院内地下道处3道供水主管道需要西移，人行道处有3处医院总水表井需要和水厂挪动水表后对接，以保障医院正常供水。\n                                                                                       三、配置规格、附件及零配件（包括专用工具）：详情见后附清单\n            \n                                                                                                             \n四、详细技术要求、参数及产品资料等：技术要求及功能参数如下：①、税务登记证、营业执照、组织机构代码或三证合一的营业执照；②、法人签字并加盖公章的委托书；③、投标人的身份证及复印件；④、失信被执行人、重大税收违法案件当事人名单、政府采购严重违法失信行为记录名单查询记录（“信用中国”及“中国政府采购网”查询记录）；⑤、近三年内参加招投标活动在经营活动中没有重大违法违纪记录的书面声明。开标时，投标企业需提供上述证件的原件或复印件加公章由评委审验。                                   \n\n                                                                                                                                                                                                                                                                                                                \n五、售后服务条件及交货日期（或工期）：施工工期：自确定中标之日起7日内完成。\n"]

{"sheet":"清单","index":1,"n_rows":7,"n_cols":5,"rows_kept":7,"merged":[[0,0,0,4]],"flags":["formulas_cached_only"]}
["供水主管道改造工程量清单"]
["序号","内容","单位","工程量","备注"]
[1,"DN150管道","米",144]
[2,"DN200管道","米",72]
[3,"挖沟槽、拆除路面及人行道并恢复","项",1]
[4,"管件、法兰等","项",1]
[5,"完成与水厂水表对接","项",1]